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LLSD AD 2.20 LOCAL TRAFFIC REGULATIONS

1. Airport regulations

At Tel-AviviSde-Dov Airport a number of local regulations
spply. The reguistions are collected in 2 manval which is
available at the AIS briefing office. This manval includes
among other, the following subjects:

a) the meaning of marking of signs:

b) information about aircrafi stands including visual
guidance systems;

¢) information about taxiing from aircraft stands includ-
ing taxiing clearance;

d) limitations in the operation of Jarge aircraft inchuding
limitations i the use of aircraft’s own power for taxi-
ing,

) helicopter operations;

f) marshaller assistance and towing assistance;

@) use of engine power exceeding idle power;

h) engine start-up and use of APU;

i) fuel spillage;

j) precautions during extreme weather conditions;

k) limits in operation due to noise abatement.

2. Taxiingto and from stands

Most parking positions on aprons 'E' and N’ (with the ex-
ception of N1-N3) are push-back type positions, i.e. they
cannot be used as self-maneuvering stands, thus may not be
entered by nircrafi using their own engine power.

Military aircraft are paried on the edges of taxiway ‘A’ ; pi-
fots are advised to exercise caution while using this taxiway.

No marshalling services are provided. Taxiing and maneu-
vering shall be the sole responsibility of the pilot. Adher-
ence to ATC instructions and OPS/AIS office directives is
mandatory.

Departing flights shall contact the TWR 10 obtain ATC
clcarance before commencing taxiing. Request for ATC
clearance may take place prior to engine stari-up clearance
Frequency 121.050 MRZ.

3. Parking areas

46 aircralt parking positions have been assigned at Tel-
AviviSde-Dyv airport. These include four positions for air-
craht up 1o DHC-7/F27 size, eight positions for aircraft up o
BNZA size, 18 positions for aircrafl up to PA3I, 12 posi-
tions for single-engined aircrafi and four helipads for helis
caplers up 10 Bell 206 size.

Parking and mooring shall be undes the sole responsibility
of the aircrafi’s owner and/or operatar. The sirport admini-
stration shall not accepe liability for any damage caused to
sireraft or property duc to careless parking and mooting of
sircraft.

10. Responsibie authority

The Tel-AviviSde-Dov airport administration, through the
Operations/AIS office, is the sole authority for any matters
concerning the parking arrangements and matters concemn-
ing the parking arrangements and procedures of aircraft at
the tirport.

at Commercial operutors

Priority in the allocation of permancnt parking positions
will be given to commercial operators. Privately owned air-
craft will be allocated permanent position according 10 their
activity, which is a2 measure of the number of monthly
movements at the aisport.

Visiting aircraft for which Tel-Aviv/Sde-Dov does not serve
as bome base, shall aot park at the airport for more than 24
Thours without obtaining prior permission from the OPS/AIS
office at the airport.

32 Smull aircraft (generel aviation)

General aviation aircrafi shall be parked in the parking ares
for small gircraft.

4. Parling area for helicopters

Parking area for helicopters consists of six marked stands
{H-11011-6).

No marshalting scrvices are provided. Taxiing and maneu-
vering shall be the solc responsibility of the pilot

8. Apron - taxiing during
winter conditions

Nil

6. Taxiing - limitations
Tnsufficicnt safety distances restrict large aircraft fram using

certain Laxiways when using thcir own power, Further in-
formation will be given to each aircraft by the TWR.

7. School and training flights
techaieal test flights - use of runways

School and training flights must only be made after permis-
sion has been obtained from Tel-Aviv/Sde-Dov AlS officc.

8. Helicopter traffic - limitation
Non-scheduted public air affic with helicopter is permitted

only after pricr approval from the Tel-Aviv/ Sde-Dov AIS
office.

9. Removal of disabled sircraft
from runways

When an airerat is wrecked on a runway, it is the duty of
the owner or user of such aircraft to have it removed as
soon as possible. 1f a wrecked aircraft is not removed from
the runway as quickly as possible by the owner or usur's

expense.

LLSD AD 2.21 NOISE ABATEMENT MONITORING & PROCEDURES

Operation limiration defined in the airport regulations.

LLSD AD 2.22 FLIGIIT PROCEDURES

General

Flights within Tel-Aviv/Sde-Dov CTR and SRZ shall be in
mmw with Controlled Visual Flight Rules (CVFR)
and in accordance with Instrument Flight Rules (IFR).

Procedures for IFR flights
within Tel-Aviv/Sde-Dov SRZ

In IMC, aircraft shall execute cloud hreak procedure.

In VMC, aircrat shall cancel IFR flight plen before enter-
ing the Tel-Aviv/Sde-Dov SRZ using the CVFR route con-
cerned.

Communication failure

In the event of communication failture, the pilot shall act in
accordance with the communication failure procedures in
ICAO Annex 2. For the Tel-aviv/Sde-Dov CTR an amiving
aircraft shall:

a) In VMC - fly over the runway and join the circuit
upon light signal from the TWR.

B)In IMC - execute
(see AD 2.6-19).

cloud break procedure

LLSD AD 2.23 ADDITIONAL INFORMATION

Bird conceatration in the vicinity of the airport

CAA

AMENDMENT 11
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